Spectrum Camera Solutions F112-NBN73023BA-BD Explosion-Proof Camera
Certified (NEC, ATEX, IECEx) for use in potentially combustible environments, this explosion proof camera delivers clear images 24/7 - event at night or under low-light conditions. The exceptional starlight sensitivity enables the explosion proof camera to work with a minimum ambient light. The extended dynamic mode provides detailed images in scenes with challenging light.
• Excellent low-light performance
• Built-in intelligent video analytics
• Intelligent Dynamic Noise Reduction to reduce bandwidth and storage
• Extended Dynamic Range mode
• Operating Temperature:
	Zone system: -50°C to +50°C 
	(USA) Class/Division system: -40°C to +50°C 
• cFMus, ATEX, IECEX, EAC, UKEX/UKCA, PESO* Pending
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.

The main unit shall be backed by a 3 years manufacturer warranty.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
Casing
IP66-rated, powdercoated aluminum chassis
Casing manufactured and certified by Spectrum Camera Solutions, LLC

Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55035, EN 55032 Class A, EN 61000-3-2, EN 61000-3-3, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-3(A)/NMB-3(A), KS C 9832 Class A, KS C 9835, RCM AS/NZS CISPR 32 Class A, VCCI Class A
Safety
CAN/CSA C22.2 No. 62368-1, IEC/EN/UL 62368-1
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78
Network
NIST SP500-267
Explosion-Proof Certifications
USA:
Class I Division 1 Groups BCD T5 Ta= -40°C to 50°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -40°C to 50°C, Type 4X, IP66
Certificate: FM18US0262X
Canada:
Class I Division 1 Groups BCD T5 Ta= -50°C to 50°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -50°C to 50°C, Type 4X, IP66
Class I, Zone 1, AEx/Ex db IIB+H2 T5 Gb Ta = -50°C to 50°C, Type 4X, IP66
Zone 21, AEx/Ex tb IIIC T85°C Db Ta = -50°C to 50°C, Type 4X, IP66
Certificate: FM18CA0126X
ATEX:
II 2 G Ex db IIB+H2 T5 Gb Ta = -50°C to 50°C, IP66
II 2 D Ex tb IIIC T85°C Db Ta = -50°C to 50°C, IP66
Certificate: FM18ATEX0073X
IECEx:
Ex db IIB+H2 T5 Gb Ta = -50°C to 50°C, IP66
Ex tb IIIC T85°C Db Ta = -50°C to 50°C, IP66
Certificate: IECEx FMG 18.0029X
INMETRO:
Ex db IIB+H2 T5 Gb
Ex tb IIIC T85°C Db IP66
Ta = -50°C to 50°C
Certificate: NCC 20.0084 X
EAC:
1Ex d IIB+H2 T5 Gb X, IP66
Ex tb IIIC T85°C Db X, IP66
Ambient Temperature Range: -50°C ≤ Tab. ≤ +50°C
Electrical Parameters: 57VDC and 7.2 W
Electrical Parameters: 12-24 VAC/VDC 25W
Certificate: RU C-US.MЮ62.B.00000/19 
Image sensor
1/2.8” CMOS

Effective Pixels
1920 (H) x 1080 (V); 2MP

Starlight sensitivity
Color: 0.0069 lx
Mono: 0.0008 lx 

High Dynamic Range 
120 dB WDR

Measured according to IEC
110 dB WDR

Video Streaming
Video compression: H.264 (MP); M-JPEG

Video Content Analysis
Analysis type: Intelligent video analytics
Alarm rules:
Any Object
Object in field
Crossing line
Entering field
Leaving field
Loitering
Following route
Idle object
Removed object
Counter
Occupancy
Crowd detection
Condition change
Similarity search
Tampering
Object filters:
Duration
Size
Aspect ratio v/h
Speed
Direction
Color
Object classes
 
Lens Option: LVF-5003C-P2713
Sensor size: 1/2.7 in.
Resolution: 3MP
Iris Range: F1.4 - close
Zoom control: Manual
Focus Control: Manual

Technical specs of camera with regard to lens
Sensor Size: 1/2.7 in.
Resolution: 1920 (H) x 1080 (V) (approx 2 MP)
Lens Mount: CS (can use C with adaptor ring)
Lens Types: Standard DC Iris auto-detect with override DC Iris Drive

General
Weight 
6.4 kg (14lb)

Dimensions 
13.85 x 7.20 x 6.01 in (352 x 183 x 153 mm)

Power 
57 VDC, 7.2 W; 12-24 VAC/VDC 25W

Storage Conditions 
-30°C to +70°C Humidity 5-98% RH (non-condensing)

Operating Conditions 
Zone system: -50°C to +50°C

(USA) Class/Division system
-40°C to +50°C
Humidity 10-100% RH (condensing)

Warranty 
3-year limited warranty, see spectrumcamera.com/warranty