Spectrum Camera Solutions F101-P1377-BD Explosion-Proof Camera
Certified (NEC, ATEX, IECEx) for use in potentially combustible environments, the lightweight camera offers high quality, high resolution images of objects and people. Featuring advanced low-light technology and advanced WDR imaging, it delivers true colors and great details in challenging light or near darkness. It includes electronic image stabilization for stable images despite vibration. And, intelligent i-CS lens technology facilitates fast and easy installation with remote zoom. Enhanced security features such as signed firmware and secure boot ensure the integrity and authenticity of the firmware. Furthermore, reduced bandwidth and storage needs with support for H.264/H.265 significantly lowers bandwidth and storage requirements.
• 30 fps in 5 MP or up to 180 fps in HDTV 720p
• Low-light technology and advanced WDR imaging
• Reduced bandwidth and storage needs supporting H.264 and H.265
• Signed firmware and secure boot
• Operating Temperature:
	Zone system: -50°C to +55°C 
	(USA) Class/Division system: -40°C to +55°C 
• cFMus, ATEX, IECEX, EAC, UKEX/UKCA, PESO* Pending
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.

The main unit shall be backed by a five years manufacturer warranty.
The product, including all its components, shall not contain any added PVC.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
Casing
IP66-rated, powdercoated aluminum chassis
Casing manufactured and certified by Spectrum Camera Solutions, LLC
Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55035, EN 61000-6-1, EN 61000-6-2, EN 55032 Class A, FCC Part 15 Subpart B Class A, ICES-3(A)/NMB-3(A), VCCI Class A, RCM AS/NZS CISPR 32 Class A
Safety
EN 62368-1
Environment
ANSI/NEMA 250 4X, ANSI/IEC/EN 60529 IP66, GOST 14254 IP66
Network
NIST SP500–267
Explosion FM Class 3600:2018, FM Class 3615:2018, FM Class 3616:2011, ANSI/ISA/EN/ABNT NBR/IEC/CAN-CSAC22.2 60079-0, ANSI/ISA/EN/ABNT NBR/IEC/CAN-CSAC22.2 60079-1, ANSI/ISA/EN/ABNT NBR/IEC/CAN-CSAC22.2 60079-31, TP TC 012, GOST 31610.0, GOST IEC 60079-1, GOST IEC 60079-31
Explosion-Proof Certifications
USA:
Class I Division 1 Groups BCD T5 Ta= -40°C to 55°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -40°C to 55°C, Type 4X, IP66
Certificate: FM18US0262X
Canada:
Class I Division 1 Groups BCD T5 Ta= -50°C to 55°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -50°C to 55°C, Type 4X, IP66
Class I, Zone 1, AEx/Ex db IIB+H2 T5 Gb Ta = -50°C to 55°C, Type 4X, IP66
Zone 21, AEx/Ex tb IIIC T85°C Db Ta = -50°C to 55°C, Type 4X, IP66
Certificate: FM18CA0126X
ATEX:
II 2 G Ex db IIB+H2 T5 Gb Ta = -50°C to 55°C, IP66
II 2 D Ex tb IIIC T85°C Db Ta = -50°C to 55°C, IP66
Certificate: FM18ATEX0073X
IECEx:
Ex db IIB+H2 T5 Gb Ta = -50°C to 55°C, IP66
Ex tb IIIC T85°C Db Ta = -50°C to 55°C, IP66
Certificate: IECEx FMG 18.0029X
INMETRO:
Ex db IIB+H2 T5 Gb
Ex tb IIIC T85°C Db IP66
Ta = -50°C to 55°C
Certificate: NCC 20.0084 X
EAC:
1Ex d IIB+H2 T5 Gb X, IP66
Ex tb IIIC T85°C Db X, IP66
Ambient Temperature: -50°C ≤ Tamb. ≤ +55°C
Electrical Parameters: Up to 57V and 10.7W
Electrical Parameters: 12-24 VAC/DC 25W
Certificate: RU C-US.MЮ62.B.00000/19

Image sensor
1/2.7” progressive scan RGB CMOS
Lens
Varifocal 3.9–10 mm, F1.5
4:3 aspect ratio:
Horizontal field of view: 75°–31°
Vertical field of view: 55°–23°
16:9 aspect ratio:
Horizontal field of view: 75°–31°
Vertical field of view: 41°–17°
Remote zoom, remote focus
Day and night
Automatically removable infrared-cut filter
Minimum illumination
5 MP 25/30 fps with advanced WDR imaging technology and low-light technology:
Color: 0.15 lux, at 50 IRE F1.5
B/W: 0.03 lux, at 50 IRE F1.5
Shutter speed
WDR: 1/33500 s to 1/5 s
No WDR: 1/5000 s to 1/5 s
Model
Manufacturer’s own chipset
Memory
1 GB RAM, 512 MB Flash
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC)
Motion JPEG
Resolution
2592x1944 (5 MP) to 160x90
2688x1512 (4 MP) to 160x90
1280x720 (HDTV 720p) to 160x90
Frame rate
Capture mode 5 MP: 25/30 fps (50/60 Hz)
Capture mode 4 MP: 25/30 fps (50/60 Hz)
Capture mode HDTV 720p: 180 fps
Video streaming
Multiple, individually configurable streams in H.264, H.265 and Motion JPEG

Controllable frame rate and bandwidth
VBR/ABR/MBR H.264/H.265
Video streaming indicator
Multi-view streaming
Up to 8 individually cropped out view areas
Image settings
Saturation, contrast, brightness, sharpness, advanced WDR imaging technology: Up to 120 dB depending on scene, white balance, day/night threshold, exposure mode, exposure zones, local contrast, tone mapping, compression, rotation: auto, 0°, 90°, 180°, 270° including corridor format, mirroring of images, dynamic text and image overlay, privacy masks, defogging, electronic image stabilization, barrel distortion correction, scene profiles: forensic, vivid, traffic overview
Pan/Tilt/Zoom
Digital PTZ
Uploadable PTZ driver (Pelco D pre-installed)
Audio streaming
Two-way, full duplex
Audio encoding
AAC LC 8/16/32/48 kHz, G.711 PCM 8 kHz, G.726 ADPCM 8 kHz, Opus 8/16/48 kHz, LPCM 48 kHz
Configurable bit rate
Audio input/output
External microphone input, line input, digital input with ring power, line output, built-in microphone (can be disabled)
Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1X (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware, secure boot
Supported protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTPS, HTTP/2, SSL/TLS, QoS Layer 3 DiffServ, FTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP™, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, RTSP, RTP, SRTP, SFTP, TCP, UDP, IGMP, RTCP, ICMP, DHCPv4/v6, ARP, SOCKS, SSH, LLDP, CDP, MQTT v3.1.1, Syslog, Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration

ONVIF® Profile G, ONVIF® Profile S, and ONVIF® Profile T, specification at onvif.org
Onscreen controls
Electronic image stabilization
Day/night shift
Defogging
Wide dynamic range
Event conditions
Analytics, shock detection, edge storage events, supervised external input, audio level, time scheduled
Event actions
Record video: SD card and network share
Upload of images or video clips: FTP, SFTP, HTTP, HTTPS, network share and email 
Pre- and post-alarm video or image buffering for recording or upload 
Notification: email, HTTP, HTTPS, TCP and SNMP trap 
PTZ: PTZ preset, start/stop guard tour 
Overlay text, external output activation, play audio clip, WDR mode, day/night mode
Data streaming
Event data
Built-in installation aids
Focus assistant, pixel counter, remote back focus, autorotation
Applications
Included
motion guard, fence guard, loitering guard video motion detection, active tampering alarm, gatekeeper
Supported
live privacy shield, perimeter defender
Support for enabling installation of third-party applications
Sustainability
PVC free
Free of hazardous brominated and chlorinated flame retardants (BFR/CFR free)
Power
Camera: Power over Ethernet (PoE) IEEE 802.3af/802.3at Type 1 Class 3, max 10.7 W, typical 5.4 W
Heater: 12-24 V DC, max 25 W 12-24 V DC is required for operating at temperatures below 0 °C (32 °F).
Connectors
2 x 3/4" NPT cable entries
RJ45 10BASE-T/100BASE-TX PoE
2-pin terminal block connector for heater 
I/O: 4-pin 2.5 mm terminal block for two configurable inputs/outputs (12 V DC output, max. load 50 mA)
3.5 mm mic/line in, 3.5 mm line out
Storage
Pre-installed 128 GB surveillance grade microSDXC card
Support for SD card encryption (AES-XTS-Plain64 256bit)
Recording to network-attached storage (NAS)
Operating conditions
-50 °C to 55°C 
US Class/Division system: -40°C to 55°C 
Humidity 10-100% RH (condensing)
Storage conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Humidity 5-95% RH (non-condensing)

Dimensions
13.85 x 7.20 x 5.97 in (352 x 183 x 152 mm)
Weight
14 lb (6.2 kg)
Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese, Polish