Spectrum Camera Solutions F101-P1378-BD Explosion-Proof Camera
Certified (NEC, ATEX, IECEx) for use in potentially combustible environments, this network camera captures excellent detailed images in 4K resolution. Featuring advanced low-light technology and advanced WDR imaging it delivers true colors and great details in challenging light or near darkness. It offers P-Iris for images with better contrast, clarity, resolution and depth of field. Designed to act as a deterrent, it includes electronic image stabilization for stable images as well as enhanced security features, barrel distortion correction, shock detection and scene profiles. Built-in reduced bandwidth and storage technology with support for H.264 and H.265 provides exceptional savings on bandwidth and storage. Plus, with CS mount and support for motorized i-CS, you can easily change lens to meet your requirements.
• 4K resolution
• Advanced low-light technology and advanced WDR imaging
• Signed firmware and secure boot
• Electronic image stabilization
• Built-in reduced bandwidth and storage technology with support for H.264 and H.265
• Operating Temperature:
	Zone system: -50°C to +55°C 
	(USA) Class/Division system: -40°C to +55°C 
• cFMus, ATEX, IECEX, EAC, UKEX/UKCA, PESO* Pending
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.

The main unit shall be backed by a minimum of three years manufacturer warranty. The manufacturer shall provide the option of extended warranty for the unit. The optional extended warranty shall be available for a total warranty period of maximum five years.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
The main unit shall be manufactured by a company that have signed and support the UN Global Compact initiative as defined by United Nations www.unglobalcompact.org/
Casing
IP66-rated, powdercoated aluminum chassis
Casing manufactured and certified by Spectrum Camera Solutions, LLC
Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55032 Class A, EN 61000-3-2, EN 61000-3-3, EN 55024, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-003 Class A, VCCI Class A, RCM AS/NZS CISPR 32 Class A, KCC KN32 Class A, KN35
Safety
IEC/EN/UL 62368-1, IS 13252
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78
Network
NIST SP500–267
Explosion-Proof Certifications
USA:
Class I Division 1 Groups BCD T5 Ta= -40°C to 55°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -40°C to 55°C, Type 4X, IP66
Certificate: FM18US0262X
Canada:
Class I Division 1 Groups BCD T5 Ta= -50°C to 55°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -50°C to 55°C, Type 4X, IP66
Class I, Zone 1, AEx/Ex db IIB+H2 T5 Gb Ta = -50°C to 55°C, Type 4X, IP66
Zone 21, AEx/Ex tb IIIC T85°C Db Ta = -50°C to 55°C, Type 4X, IP66
Certificate: FM18CA0126X
ATEX:
II 2 G Ex db IIB+H2 T5 Gb Ta = -50°C to 55°C, IP66
II 2 D Ex tb IIIC T85°C Db Ta = -50°C to 55°C, IP66
Certificate: FM18ATEX0073X
IECEx:
Ex db IIB+H2 T5 Gb Ta = -50°C to 55°C, IP66
Ex tb IIIC T85°C Db Ta = -50°C to 55°C, IP66
Certificate: IECEx FMG 18.0029X
INMETRO:
Ex db IIB+H2 T5 Gb
Ex tb IIIC T85°C Db IP66
Ta = -50°C to 55°C
Certificate: NCC 20.0084 X
EAC:
1Ex d IIB+H2 T5 Gb X, IP66
Ex tb IIIC T85°C Db X, IP66
Ambient Temperature: -50°C ≤ Tamb. ≤ +55°C
Electrical Parameters: Up to 57V and 10.7W
Electrical Parameters: 12-24 VAC/DC 25W
Certificate: RU C-US.MЮ62.B.00000/19

Image sensor
1/1.8” progressive scan RGB CMOS
Lens
IR corrected, CS-mount lens, P-Iris
Varifocal 3.9–10 mm, F1.5
Horizontal field of view: 119°–45°
Vertical field of view: 62°–25°
Day and night
Automatically removable infrared-cut filter
Minimum illumination
4K 25/30 fps with advanced WDR imaging technology and low-light technology:
Color: 0.15 lux, at 50 IRE F1.5
B/W: 0.03 lux, at 50 IRE F1.5
Shutter speed
1/8500 s to 1/5 s
System on Chip model
Manufacturer’s own chipset
Memory
2 GB RAM, 512 MB Flash
Compute capabilities
Machine learning processing unit (MLPU)
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC)
Motion JPEG
Resolution
3840x2160 (4K) to 160x90
Frame rate
25/30 fps (50/60 Hz) in all resolutions
Video streaming
Multiple, individually configurable streams in H.264, H.265, and Motion JPEG

Controllable frame rate and bandwidth
VBR/ABR/MBR H.264/H.265
Video streaming indicator
Multi-view streaming
Up to 8 individually cropped out view areas
Image settings
Saturation, contrast, brightness, sharpness, advanced WDR imaging technology: Up to 120 dB depending on scene, white balance, day/night threshold, exposure mode, exposure zones, local contrast, tone mapping, compression, orientation: auto, 0°, 90°, 180°, 270° including corridor format, mirroring of images, dynamic text and image overlay, privacy masks, defogging, electronic image stabilization, barrel distortion correction, scene profiles: forensic, vivid, traffic overview
Pan/Tilt/Zoom
Digital PTZ
Uploadable PTZ driver (Pelco D pre-installed)
Audio streaming
Two-way, full duplex
Audio encoding
AAC LC 8/16/32/48 kHz, G.711 PCM 8 kHz, G.726 ADPCM 8 kHz, Opus 8/16/48 kHz, LPCM 48 kHz
Configurable bit rate
Audio input/output
External microphone input, line input, digital input with ring power, line output, built-in microphone (can be disabled), automatic gain control
Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1X (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware, secure boot
Supported protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTPS, HTTP/2, TLS, QoS Layer 3 DiffServ, FTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP™, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, RTSP, RTP, SRTP, SFTP, TCP, UDP, IGMPv1/v2/v3, RTCP, ICMP, DHCPv4/v6, ARP, SOCKS, SSH, LLDP, CDP, MQTT v3.1.1, Syslog, Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration

ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S, and ONVIF® Profile T, specification at onvif.org
Onscreen controls
Electronic image stabilization
Day/night shift
Defogging
Wide dynamic range
Event triggers
Analytics, shock detection, edge storage events, supervised external input, audio level, time scheduled
MQTT subscribe
Event actions
MQTT publish
Record video: SD card and network share
Upload of images or video clips: FTP, SFTP, HTTP, HTTPS, network share and email 
Pre- and post-alarm video or image buffering for recording or upload 
Notification: email, HTTP, HTTPS, TCP and SNMP trap 
PTZ: PTZ preset, start/stop guard tour 
Overlay text, external output activation, play audio clip, WDR mode, day/night mode
Data streaming
Event data
Built-in installation aids
Focus assistant, pixel counter, remote back focus, autorotation
Object Analytics
Object classes: humans, vehicles
Trigger conditions: line crossing, object in area
Up to 10 scenarios
Metadata visualized with color-coded bounding boxes
Polygon include/exclude areas
Perspective configuration
ONVIF Motion Alarm event
Applications
Included
object analytics
video motion detection, active tampering alarm, audio detection
Supported
live privacy shield
Support for additional applications if the device is used with compatible accessories. For more information, contact your distributor partner.
Support for enabling installation of third-party applications
Sustainability
PVC free
Free of hazardous brominated and chlorinated flame retardants (BFR/CFR free)

Power
12–28 V DC, max 10.5 W, typical 6.1 W
Power over Ethernet (PoE) IEEE 802.3af/802.3at Type 1 Class 3, max 10.7 W, typical 6.2 W
Power redundancy
Heater: 12-24 VAC/VDC, 25W
Connectors
RJ45 10BASE-T/100BASE-TX/1000BASE-T
I/O: 6-pin 2.5 mm terminal block, for 2 supervised alarm inputs and 2 outputs
RS485/RS422, 2 pcs, 2 pos, full duplex, terminal block
DC input, terminal block, 3.5 mm mic/line in, 3.5 mm line out
i-CS connector (compatible with P-Iris and DC-iris)
Security lock slot
manufacturer’s supported connector
Storage
Support for microSD/microSDHC/microSDXC card
Support for SD card encryption (AES-XTS-Plain64 256bit)
Support for recording to network-attached storage (NAS)
Operating conditions
-50 °C to 55°C 
US Class/Division system: -40°C to 55°C 
Humidity 10-100% RH (condensing)
Storage conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Humidity 5-95% RH (non-condensing)
Dimensions
13.85 x 7.20 x 5.97 in (352 x 183 x 152 mm)
Weight
14 lb (6.2 kg)
Optional lenses
Lens CS 4-10 mm F0.9 P-Iris
Lens i-CS 3.9-10 mm F1.5 8 MP
Lens i-CS 9-50 mm F1.5 8 MP
Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese, Polish