Spectrum Camera Solutions F112-NBN80052BA-BD Explosion-Proof Camera
Certified (NEC, ATEX, IECEx) for use in potentially combustible environments, this explosion proof camera delivers clear images 24/7 - event at night or under low-light conditions. The explosion-proof camera delivers multi-megapixel full-color video in near darkness, and delivers detailed monochrome images where other cameras show no image at all.
• 5 MP  (3K) high detail at fast speeds (30 fps)
• Built-in intelligent video analytics
• Low network strain and storage costs
• Operating Temperature:
	Zone system: -50°C to +50°C 
	(USA) Class/Division system: -40°C to +50°C 
• cFMus, ATEX, IECEX, EAC, UKEX/UKCA, PESO* Pending
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.

The main unit shall be backed by a 3 years manufacturer warranty.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
Casing
IP66-rated, powdercoated aluminum chassis
Casing manufactured and certified by Spectrum Camera Solutions, LLC

Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55035, EN 55032 Class A, EN 61000-3-2, EN 61000-3-3, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-3(A)/NMB-3(A), KS C 9832 Class A, KS C 9835, RCM AS/NZS CISPR 32 Class A, VCCI Class A
Safety
CAN/CSA C22.2 No. 62368-1, IEC/EN/UL 62368-1
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78
Network
NIST SP500-267
Explosion-Proof Certifications
USA:
Class I Division 1 Groups BCD T5 Ta= -40°C to 50°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -40°C to 50°C, Type 4X, IP66
Certificate: FM18US0262X
Canada:
Class I Division 1 Groups BCD T5 Ta= -50°C to 50°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -50°C to 50°C, Type 4X, IP66
Class I, Zone 1, AEx/Ex db IIB+H2 T5 Gb Ta = -50°C to 50°C, Type 4X, IP66
Zone 21, AEx/Ex tb IIIC T85°C Db Ta = -50°C to 50°C, Type 4X, IP66
Certificate: FM18CA0126X
ATEX:
II 2 G Ex db IIB+H2 T5 Gb Ta = -50°C to 50°C, IP66
II 2 D Ex tb IIIC T85°C Db Ta = -50°C to 50°C, IP66
Certificate: FM18ATEX0073X
IECEx:
Ex db IIB+H2 T5 Gb Ta = -50°C to 50°C, IP66
Ex tb IIIC T85°C Db Ta = -50°C to 50°C, IP66
Certificate: IECEx FMG 18.0029X
INMETRO:
Ex db IIB+H2 T5 Gb
Ex tb IIIC T85°C Db IP66
Ta = -50°C to 50°C
Certificate: NCC 20.0084 X
EAC:
1Ex d IIB+H2 T5 Gb X, IP66
Ex tb IIIC T85°C Db X, IP66
Ambient Temperature Range: -50°C ≤ Tab. ≤ +50°C
Electrical Parameters: 57VDC and 7.2 W
Electrical Parameters: 12-24 VAC/VDC 25W
Certificate: RU C-US.MЮ62.B.00000/19 
Image sensor
1/1.8” CMOS

Effective Pixels
6.1MP

Sensor
Bosch NBN-80052-BA

Video Performance - Dynamic Range
5.5 MP (4:3) mode - 97 dB WDR (97 + 16 dB with IAE)
5 MP (16:9) mode - 97 dB WDR (97 + 16 dB with IAE)
1080p mode - 103 dB WDR (103 + 16 dB with IAE)

Color 5MP mode
0.0121lx

Color 1080p mode
0.00825 lx

Mono 5MP mode
0.004 lx

Mono 1080P mode
0.00275

Video compression
H.264 (MP); M-JPEG

Streaming
Multiple configurable streams in H.264 and M-JPEG, configurable frame rate and bandwidth. Region of interest (ROI)

Overall IP Delay
Min. 120 ms, max. 340 ms

GOP Structure
IP, IBP, IBBP

Encoding interval
1 to 30 [25 fps]

Encoder regions
Up to 8 areas with encoder quality settings per area

Video resolution
5MP (16:9) - 2992 x 1680

Video content analysis type
Intelligent Video Analytics

Configurations
Silent VCA/ Profile 1/ Profile 2/ Event triggered/ scheduled

Alarm rules (combinable)
Any object
Object in field
Crossing line
Entering field
Leaving field
Loitering
Following route
Idle object
Removed Object
Counter Occupancy
Crowd detection
Condition Change
Similarity search
Tampering

Object filters
Duration
Size
Aspect ratio
Color
Object classes

Lens Mount
CS mount (C-mount with adapter ring)

Lens connector
Standard 4-pin DC iris connector / P-iris connector

Focus control
Motorize back-focus adjustment

Lens option: LV-5005C-C4109
Sensor size: 1/1.8 inch
Resolution: 5 MP
Iris range: F1.6 - F8
Focal length: 4.1mm 9mm
Lens mount: CS
Lens connector: 4 Pin DC control
Dimensions: 62.9mm x 66.6
Zoom Control: Manual
Focus Control: Manual

Technical Specs of camera with regard to lens
Sensor Size: 1/1.8”
Resolution: 5MP
Lens Mount: CS (can use C with adapter ring)
Lens Connector: Standard 4 pin DC iris connector
Lens Types: DC iris and P-iris* control

Weight 
6.4 kg (14lb)

Dimensions 
13.85 x 7.20 x 6.01 in (352 x 183 x 153 mm)

Power 
57 VDC, 9W; 12-24 VAC/VDC 25W

Storage Conditions 
-30°C to +70°C Humidity 5-98% RH (non-condensing)

Operating Conditions 
Zone system: -50°C to +50°C

(USA) Class/Division system
-40°C to +50°C
Humidity 10-100% RH (condensing)

Warranty 
3-year limited warranty, see spectrumcamera.com/warranty